**SAS 500 / 550 se­mi-cou­pler bar with he­xa­go­nal cou­pler**

Rein­for­cing cou­pling sys­tem to con­nect bars of the sa­me dia­me­ter, if the con­nec­ting bar is not ro­ta­table, e.g. in the area of co­lumns with ben­ding rein­force­ment.

Con­sis­ting of:
1 he­xa­go­nal cou­pler, long (T3010), 1 lock nut (T2003), 1 saw tip, 1 end cap (T5025), 1x lo­cking/screwing
SAS 500 / 550 sys­tem ac­cor­ding to ap­pro­val no. Z-1.1-58, Z-1.5-174, Z-1.1-106, Z-1.5-173. Ma­nu­fac­tu­rer: Stahl­werk Anna­hütte, D-83404 Ham­merau
In­stal­la­ti­on as spe­ci­fied by the struc­tu­ral en­gi­neer.

Dia­me­ter of the rein­force­ment: \_\_\_\_\_\_\_mm